Fiber optic Media converter



Key Features

* Supported 10/100/1000Base-T Ethernet
* 케이블 MDI/MDI-X 자동감지
* Flow control 지원

|  |
| --- |
| Specifications |
| Model  | SL-G2000TS | SL-G2000TL |
| Interface | 1x 10/100/1000Mbps RJ45 Port |
| 1x 1Gb SC type Fiber Optic Port |
| Standards | IEEE802.3 10Base-T |
| IEEE802.3u 100Base-T |
| IEEE802.3ab 1000BASE-T |
| IEEE802.3z 1000BASE-FX |
| Wavelength | 850nm / Multimode | 1310nm / Singlemode |
| Distance | 224M(62.um) / 550M(50um) | 20KM |
| Fiber Connector | SC Duplex |
| Dimension | 26(H) x 70(W) x 94(D)mm |
| Working environment | Working Temperature: -0~50℃ |
| Storing Temperature: -10 ~ 50℃ |
| Humidity: 10~90% (No condenser) |
| Input Power | DC5V 1A |
| Warranty | 3years (1년무상, 2년유상) |

**Order info**

|  |  |
| --- | --- |
| **SL-G2000TL** | 10/100/1000Base-T to 1000Base-FX Duplex Singlemode Media converter |
| **SL-G2000TS** | 10/100/1000Base-T to 1000Base-FX Duplex Multimode Media Converter |