

Key Features

* Compatible IEEE802.3af/at PoE+ 30W
* Automatic detection and protection of Non-Standard Ethernet terminals
* IP30 Protection Class, DIN35 rail Mounting
* Industrial design protection grade 4, -40 to 75 ° C operating temperature

|  |  |
| --- | --- |
| Specifications | |
| Model | SL-G6042PF |
| Interface | 4x 10/100/1000T PoE |
| 2x 1GE SFP Port |
| Standards | 802.3 10Base-T |
| 802.3u 100Base-T |
| 802.3ab 1000Base-T |
| 802.3x flow control |
| 802.3z 1000Base-X |
| 802.3af/at Power ethernet compliant |
| Bandwidth | 12Gbps |
| Mac address | 2K MAC |
| PoE Spec | PoE Standard IEEE802.3af/at |
| Per Port Max 30W |
| Power pin : 1/2(+),3/6(-) |
| Industry standard | EN61000-4-2(ESD) |
| EN61000-4-4(EFT) |
| EN61000-4-5(Surge) |
| IEC60068-2-27(shock) |
| IEC60068-2-32(free fall) |
| IEC60068-2-6(vibration) |
| Dimension | 280(W) x 180(D) x 44(H)mm |
| Working environment | Working Temperature: -40~75° C |
| Storing Temperature: -40 ~ 85° C |
| Humidity: 5~95% (No condenser) |
| Input Power | DC48~55V / 3pin terminal block, |
| Power consumption | Max 150W |
| Warranty | 3years (1년무상, 2년유상) |
|  |  |