

SL-POE3108GSFP

Key Features

* IEEE802.3af/at PoE Standard compatible
* Automatic detection and protection of Non-Standard Ethernet terminals
* 2Port Gigabit Uplink Port
* Save up to 83% Power Green Technology

|  |  |
| --- | --- |
| Specifications | |
| Model | SL-POE3108GSFP |
| Interface | 8x 10/100/1000T PoE |
| 1x Gigabit RJ45 Port, 1x 1GE SFP Port |
| Standards | 802.3 10Base-T |
| 802.3u 100Base-T |
| 802.3ab 1000Base-T |
| 802.3x flow control |
| 802.3z 1000Base-X |
| 802.3af/at Power ethernet compliant |
| Bandwidth | 20Gbps |
| Mac address | 8K MAC |
| PoE config | Support Per Port Max 30W |
| PoE Power Max. 130W |
| 1/2(+), 3/6(-) Endspan |
| Dimension | 210(W) x 140(D) x 45(H)mm |
| Working environment | Working Temperature: 0~40℃ |
| Storing Temperature: -20 ~ 55℃ |
| Humidity: 10~90% (No condenser) |
| Input Power | 100~ 240VAC 50/60Hz, |
| Power consumption | Max 150W |
| Warranty | 3years (1년무상, 2년유상) |
|  |  |