SL-POE504AE



Key Features

* Supported IEEE802.3af/at
* Automatic detection and protection of Non-Standard Ethernet terminals
* Up to 30W Per Port Power
* Extend Mode to support 250Meter Long Distance (cat.6)
* Watchdog function & Power indicator supported

|  |  |
| --- | --- |
| Specifications | |
| Model | SL-POE504AE |
| Interface | 4x 10/100TP PoE |
| 1x 10/100TP Uplink Port |
| Standards | 802.3 10Base-T |
| 802.3u 100Base-T |
| 802.3x flow control |
| 802.3af/at Power ethernet compliant |
| Bandwidth | 1.6Gbps |
| Mac address | 1K MAC |
| Function Switch | All off : Standard Mode |
| E : “ON” Extender Mode Max 250Meter(10Mbps), Vlan Mode |
| D : “ON” Watchdog AI-self healing function |
| P : “ON” Power indicator Monitor $ POE priority |
| PoE Parameter | Support Per Port Max 30W |
| PoE Budget: 60W |
| 1/2(+), 3/6(-) Endspan |
| Dimension | 118(W) x 95(D) x 28(H)mm |
| Working environment | Working Temperature: -20~55℃ |
| Storing Temperature: -40~75℃ |
| Humidity: 10~90% (No condenser) |
| Input Power | 48VDC 1.25A, |
| Power consumption | Max 65W |
| Warranty | 3years (1년무상, 2년유상) |
|  |  |