**SL-POE510G**



Key Features

* IEEE802.3af Backward compatible
* Automatic detection and protection of Non-Standard Ethernet terminals
* Up to 30W Per Port Power
* 2Port Gigabit Uplink Ports
* PoE Port Extend Mode Support Max 250Meter

|  |  |
| --- | --- |
| Specifications | |
| Model | SL-POE510G |
| Interface | 8x 10/100M RJ45 PoE Port |
| 2x Gigabit RJ45 Port |
| Standards | 802.3 10Base-T |
| 802.3u 100Base-T |
| 802.3ab 1000Base-T |
| 802.3x flow control |
| 802.3af/at Power ethernet compliant |
| Bandwidth | 16Gbps |
| Mac address | 4K MAC |
| Dip Switch | |
| N | 일반적인 네트워크 전송모드 |
| V | Port isolation (PoE포트끼리 통신차단) |
| S | 장거리전송모드 ON: 최대전송거리 200Meter(10Mbps), Off: 100Meter(100Mbps) |
| PoE Parameter | Support Per Port Max 30W |
| PoE Power Max 120W |
| 1/2(+), 3/6(-) Endspan |
| Dimension | 210(W) x 150(D) x 35(H)mm , Rackmount support |
| Working environment | Working Temperature: -10~55 |
| Storing Temperature: -40 ~ 75 |
| Humidity: 10~90% (No condenser) |
| Power | 100~ 240VAC 50/60Hz, 최대 소비전력 120W |
| Warranty | 3years (1년무상, 2년유상) |
|  |  |