**SL-POE5604E**



Key Features

* Supported IEEE802.3af/at
* Automatic detection and protection of Non-Standard Ethernet terminals
* Up to 30W Per Port Power & 1Port Max 60W
* Extend Mode to support 250Meter Long Distance (cat.6)
* Watchdog function

|  |  |
| --- | --- |
| Specifications | |
| Model | SL-POE5604E |
| Interface | 4x 10/100TP PoE |
| 2x 10/100TP Uplink Port |
| Standards | 802.3 10Base-T |
| 802.3u 100Base-T |
| 802.3x flow control |
| 802.3af/at Power ethernet compliant |
| Bandwidth | 1.6Gbps |
| Mac address | 1K MAC |
| Function Switch | Default Watchdog function : v1 on, v2 off |
| N : 일반 표준모드 |
| V : Port isolation 포트끼리 개별통신(서로통신불가1~4번) |
| S : Extend Mode Max 250Meter(작동시 10Mbps PoE포트) |
| PoE Parameter | Support Per Port Max 30W |
| PoE Budget: 70W |
| 1/2(+), 3/6(-) Endspan |
| Dimension | 190(W) x 130(D) x 35(H)mm |
| Working environment | Working Temperature: -10~55℃ |
| Storing Temperature: -40~75℃ |
| Humidity: 10~90% (No condenser) |
| Input Power | AC100~240VAC, |
| Power consumption | Max 80W |
| Warranty | 3years (1년무상, 2년유상) |
|  |  |